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HDNet Movies and AXS TV File Delivery Information
Effective June 1, 2022


File Specifications
Format Name: MPEG HD422 (XDCAM HD) 
Container: MXF 
Operational Pattern: OP-1A  
Video Coding: MPEG-2 422P@HL 
Bit Depth: 8 
Color Sampling: 4;2:2
Frame Size: 1920 x 1080
Frame Rate: 29.97 
Scanning Type: Interlace
Video Bit Rate: 50 Mbps (CBR)
Insert after Frame Rate
Field Order: Upper First
Audio: Channel 1 and channel 2 – Stereo or Mono (native to movie); 5.1 Surround Sound Audio Mapping:
Ch. 1 – Front Left
Ch.2 – Front Right
Ch.3 – Centre
Ch.4 – LFE (ie. bass)
Ch. 5 – Rear Left
Ch. 6 – Rear Right)
Captions:  embedded on 608/708 (please send separate .scc file)

Tech Contact: ittechs@axs.tv
Administrative Contact:  Diana Ritter, dritter@hdnetmovies.com
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